PANASONIC WV-S1536L FIXED NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	Panasonic i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	PANASONIC WV-S1536L FIXED NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Fixed Camera shall deliver H.265 stream and H.264 stream. 

2.	The Fixed Camera shall produce a resolution of 1920x1080 pixels at up to 60 fps with a 16:9 aspect ratio, 1280x960 pixels at up to 30 fps with a 4:3 aspect ratio, and 2048x1536 pixels at up to 15 fps with a 4:3 aspect ratio.

3.	The Fixed Camera shall utilize an approximate 1/2.8 type high sensitivity CMOS image sensor. 

4.	The Fixed Camera shall built-in AI engine to enable analytical applications on network edge. Built-in AI engine supports the detecting suspicious changes in captured scenes, optimizing the image settings of the camera (based on captured scene analysis) for better image usability, and optimizing video compression through captured scenes to save bandwidth.

5.	The Fixed Camera shall enables to install the optional analytics applications with including developed by third party companies using this camera's SDK.

6.	The Fixed Camera shall feature a 144dB wide dynamic range based on Enhanced Super Dynamic and built-in AI engine and Adaptive Black Stretch technology (ABS). 

7.	The Fixed Camera shall produce a color image with a minimum illumination of 0.007 lux and a monochrome image with 0.006 lux at F1.3, shutter speed of 1/30s. 

8.	The Fixed Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 70m (230 feet) irradiation distance.
9.	
10.	The Fixed Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

11.	The Fixed Camera shall be equipped with AI intelligent auto mode which is the technology for shooting license plate and person’s face more clearly.

12.	The Fixed Camera shall be equipped with GOP controls including smart facial coding and frame control and it reduce bit rate by controlling the image quality of still areas, moving areas, and faces with AI engine.   

13.	The Fixed Camera shall be equipped with corridor mode enables the capture of 
a more vertically-oriented area than the normal format would allow.

14.	The Fixed Camera shall produce encrypted stream.

15.	The Fixed Camera shall realize SSL / TLS communication with CA certificate. 

16.	The Fixed Camera shall be rated to IK10 vandal resistance.

17.	The Fixed Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress.

18.	A user shall be able to view video on a PC using a browser.

19.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

20.	The Fixed Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

21.	The Fixed Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something or the camera direction is changed to shoot a different subject.

22.	The Fixed Camera shall have Fog compensation function.

23.	The Fixed Camera shall have High light compensation (HLC) function.

24.	The Fixed Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

25.	The Fixed Camera shall provide up to eight (8) areas of electronic privacy masking. 

26.	The Fixed Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

27.	The Fixed Camera shall have a microSD memory card slot that supports microSD, microSDHC and microSDXC memory card for local storage. 

28.	The Fixed Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

29.	The Fixed Camera shall have f three (3) alarm sources of terminal input, VMD, command alarm, and audio detection alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and Panasonic alarm protocol output.

30.	The Fixed Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/2.8 type CMOS image sensor
2.	Effective Pixels                  Approx. 2.1 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.007 lux (30IRE, F1.3, Maximum shutter: Off(1/30s), AGC: 11)
0.009 lux (50IRE, F1.3, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.0 lux (with IR LED on)
0.005 lux (50IRE, F1.3, Maximum shutter: Off(1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		144 dB max. (Super Dynamic: On)
7.	Built-in IR illumination
a.	Irradiation distance	Approx. 70m (230 feet) (30IRE) *Converted value
Approx. 50m (164 feet) (30IRE)

C.	LENS
1.	Vari-Focal Length		2.9 - 9mm (1/8 - 11/32 inches)
2.	Max. Aperture Ratio	1:1.3 (WIDE) - 1:2.5 (TELE)
3.	Angular Field of View
a.	16:9 aspect ratio	H: 37° (TELE) - 117° (WIDE)
V: 21° (TELE) -   62° (WIDE)
b.	4:3 aspect ratio	H: 27° (TELE) -   82° (WIDE)
V: 20° (TELE) -   62° (WIDE)
4.	Adjusting Angle
a.	Ceiling mounting	Horizontal angle: ±180°
Vertical (TILT) angle: 0° to 100°
Azimuth (YAW) angle: -190° to +100°
b.	Wall mounting	Horizontal angle: ±100°
Vertical (TILT) angle: ±100°
Azimuth (YAW) angle: -190° to +100°
5.	Focus Adjustment		Motorized
6.	Optical Zoom Ratio	3.1x (Motorized)

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio 
1920x1080, 1280x720, 640x360, 320x180
b.	4:3 aspect ratio (30 fps)
1280x960, VGA, QVGA
c.	4:3 aspect ratio (15 fps)
2048x1536, 1280x960, VGA, QVGA
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort 
b.	Frame Rate		(60fps mode) 1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 / 60 fps
(30fps mode) 1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps
(50fps mode) 1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 / 50 fps
(25fps mode) 1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps
c.	Bit Rate/Client	64k / 128k / 256k / 384k / 512k / 768k / 1,024k / 1,536k / 2,048k
 / 3,072k / 4,096k / 6,144k / 8,192k / 10,240k / 12,288k
 / 14,336k / 16,384k / 20,480k / 24,576k bps
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate            Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull(Refresh Interval)/ Push(MJPEG)
5.	Smart Coding
a.	GOP(Group of picture) control
Off/ Low (Variable GOP 1s-8s)/ Mid (Variable GOP 4s-16s)
/Advanced (Fixed GOP 60 seconds with 1 second Key frame)
/Frame rate control (Variable GOP 4s-16s with frame rate control)
*Advanced and Frame rate control are only available with H.265.
b.	Smart VIQS		On(High)/On(Low)/Off
c.	Smart P-picture control
On/Off

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, 
G.711 64kbps, 
AAC-LC 128k / 96k /  64 kbps
b.	Audio Mode		OFF / Mic (Line) input / Audio output / Interactive (Half duplex) /
Interactive (Full duplex)

F.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off
The level can be set in the range of 0 to 8.
 (Only when AI intelligent auto / auto contrast adjust: Off)
5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation)
 /Off 
The level can be set in the range of 0 to 31.
(Only when Super Dynamic and Intelligent Auto is Off)
6.	Shutter Speed		1/10000 to 1/60 s (60fps mode)
1/10000 to 1/50 s (50fps mode)
1/10000 to 1/30 s (30fps mode)
1/10000 to 1/25 s (25fps mode)
7.	Day & Night		Off/ On(IR Light Off)/ On(IR Light On)/ Auto1(IR Light Off)/
Auto2(IR Light On)/ Auto3(SCC)
8.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
9.	Video Motion Detection	On / Off, 4 areas
10.	Scene Change Detection(SCD)
On / Off, 1 area
11.	Audio Detection		On / Off, Selectable from Gunshot, Yell, Vehicle horn, Glass break
12.	Privacy Zone		On / Off, Up to 8 zones
13.	Camera Title (OSD)	On / Off, Up to 40 characters (alphanumeric characters, marks)

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, SMTP, DNS, NTP,
SNMPv1/v2/v3, DHCPv6, RTP, MLD, ICMP, ARP, 
IEEE 802.1X, DiffServ
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, RTSP, RTP, 
RTP/RTCP, SMTP, DHCP, DNS, DDNS, NTP, SNMPv1/v2/v3, 
UPnP, IGMP, ICMP, ARP, IEEE 802.1X, DiffServ, SRTP
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

H.	INTERFACE
1.	Monitor Output		VBS : 1.0 V [p-p] / 75 ohm, NTSC / PAL composite, Pin jack
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack
3.	Audio Output		ø3.5 mm stereo mini jack (monaural output) 
4.	External I/O Terminals	ALARM IN 1 (Alarm input 1/Black & white input/
Auto time adjustment input) (x1)
 ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)
ALARM IN 3 (Alarm input 3/ AUX OUT) (x1)
5.	SD memory card slot	1 slot, microSD/microSDHC/microSDXC

I.	ELECTRICAL
1.	Power Source		DC 12V/480mA, 
PoE (IEEE802.3af compliant) DC 48V 190mA
2.	Power Consumption	Approx. 8.5W (DC 12V), Approx. 9.1W (PoE) (Class 0 device)

J.	SAFETY / EMC
1.	Safety			UL (UL62368-1), c-UL (CSA C22.2 No.62368-1), CE, 
IEC62368-1
2.	EMC 			FCC (Part15 ClassA), ICES-003 ClassA, EN55032 ClassB,
EN55035

K.	MECHANICAL
1.	Dimensions 		133 mm (W) × 133 mm (H) × 383 mm (D)
{5-1/4inches (W) × 5-1/4 inches (H) × 15-3/32 inches (D)}
2.	Weight			Approx. 2.4kg {5.3 lbs}
3.	Construction material
a.	Main body		Aluminum die cast and resin
b.	Front panel		Polycarbonate resin
c.	Outer fixing screws	Stainless steel (Corrosion-resistant treatment)
4.	Finish
a.	Main body		i-PRO white
b.	Front panel		Clear

L.	ENVIRONMENTAL
1.	Ingress Resistance	IP66 (IEC60529), Type 4X (UL50E), NEMA 4X compliant
2.	Vandal Resistance	IK10 (IEC 62262)
3.	Wind Resistance               Up to 40 m/s {approx. 89 mph}
4.	Operating Temperature	-30°C - +60°C (-22°F - 140°F)
5.	Operating Humidity	 10% - 100% (no condensation)

M.	Optional Extension Software
1.	AI Video Motion Detection	
WV-XAE200W
2.	AI Privacy Guard		WV-XAE201W