PANASONIC WV-U1132A FIXED NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

１	PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	Panasonic i-PRO Sensing Solutions Co., Ltd.

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	PANASONIC WV-U1132A FIXED NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Fixed Camera shall deliver H.265/H.264 stream. 

2.	The Fixed Camera shall utilize an approximate 1/3 type high sensitivity CMOS image sensor.

3.	The Fixed Camera shall produce a resolution of 1920×1080 pixels at up to 30 fps with a 16:9 aspect ratio. 

4.	The Fixed Camera shall be equipped 2.5 times optical motorized zoom and motorized focus.

5.	The Fixed Camera shall feature a 120dB wide dynamic range based on Enhanced Super Dynamic. 

6.	The Fixed Camera shall produce a color image with a minimum illumination of 0.1 lux and a monochrome image with 0.04 lux at F2.0, shutter speed of 1/30s and AGC 11. 

7.	The Fixed Camera shall generate multiple simultaneous video streams of up to three (3) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

8.	The Fixed Camera shall be equipped with intelligent auto mode, the technology for shooting license plate and person’s face more clearly.

9.	The Fixed Camera shall be equipped with GOP control included frame rate control which control an image quality of a stationary area, a moving area, as bitrate reducing technology.

10.	The Fixed Camera shall with corridor mode enables the capture of a more vertically-oriented area than the normal format would allow. 
                                                                                        
11.	The Fixed Camera shall realize SSL / TLS communication. 

12.	A user shall be able to view video on a PC using a browser.

13.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

14.	The Fixed Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

15.	The Fixed Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something or the camera direction is changed to shoot a different subject.

16.	The Fixed Camera shall have Fog compensation function.

17.	The Fixed Camera shall have High light compensation (HLC) function.

18.	The Fixed Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

19.	The Fixed Camera shall provide up to eight (8) areas of electronic privacy masking. 

20.	The Fixed Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

21.	The Fixed Camera shall have a SD memory card slot that supports microSD, microSDHC and microSDXC memory card for local storage. 

22.	The Fixed Camera shall have three (3) alarm sources of SCD alarm, VMD, and command alarm that activate the processes such as microSDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, and Panasonic alarm protocol output.

23.	The Fixed Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/3 type CMOS image sensor
2.	Effective Pixels                  Approx. 2.4 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.1 lux  (F2.0, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.04 lux (F2.0, Maximum shutter: Off (1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		120 dB typ. (Super Dynamic: On)

C.	Lens
1.	Vari-Focal Length		2.9 ~ 7.3 mm (1/8 ~ 9/32 inches)
2.	Max. Aperture Ratio	1 : 2.0 (WIDE) ~ 1 : 3.0 (TELE)
3.	Angular Field of View
a.	16:9 aspect ratio	H: 44° (TELE) - 102° (WIDE)
V: 24° (TELE) -   56° (WIDE)
b.	  4:3 aspect ratio	H: 36° (TELE) -   83° (WIDE)
V: 27° (TELE) -   63° (WIDE)
4.	Focus Adjustment		Motorized
5.	Optical Zoom Ratio           2.5x (Motorized)

D.	VIDEO
1.	Compression Format	H.265/ H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio 
1920 x 1080 / 1280 x 720 / 640 x 360 / 320 x 180 
b.	 4:3 aspect ratio
1600 x 1200 / 1280 x 960 /  VGA / QVGA
3.	H.265 /H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps (30fps)
                                  1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps (25fps)
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 / 20480 / 24576 kbps

d.	Image Quality	
i.	Constant bit rate	Motion priority / Normal / Quality priority
ii.	Frame rate            Motion priority / Normal / Quality priority
iii.	Best effort	Motion priority / Normal / Quality priority
iv.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
H.265/ H.264             Off / On (Low) / On (Mid) / On (Advanced) / 
On (Frame rate control)
b.	Auto VIQS                 On / Off

E.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Fog compensation	On / Off   The level can be set in the range of 0 to 8.
  (Only when intelligent auto / auto contrast adjust: Off)
4.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off (Only when Super Dynamic and intelligent Auto is off)
5.	Maximum Gain (AGC)       The level can be set in the range of 0 to 11.
6.	Shutter Speed		1/10000 to 16/30 s (30fps mode)
7.	Day & Night		Off/On/Auto1(Normal)/Auto2(IR Light)/Auto3(SCC)
8.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
9.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
10.	Scene Change Detection(SCD)     
On / Off, 1 area,
11.	Privacy Zone		 On / Off, Up to 8 zones
12.	Camera Title (OSD)	 Up to 20 characters(alphanumeric characters, marks)
13.	Digital Zoom                       x4

F.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, IEEE 802.1X, DiffServ
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, 
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ
4.	Max. User access		Up to 14 users(Depends on network conditions)

5.	Mobile Terminal Compatibility
iPad / iPhone (OS 8 or later）, AndroidTM mobile terminals

G.	INTERFACE
1.	SD memory card slot	1 slot, microSD/SDHC/SDXC

H.	ELECTRICAL
1.	Power Source		PoE (IEEE802.3af compliant) Device
DC48V/90mA 
2.	Power Consumption	Approx. 4.3W (Class 2 device)

I.	SAFETY / EMC
1.	Safety			UL (UL60950-1), c-UL (CSA C22.2 No.60950-1), CE, 
				IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024

J.	MECHANICAL
1.	Dimensions 		59 mm x 49 mm x 116 mm
{2-5/16 inches x 1-15/16 inches x 4-9/16 inches}
                                          Excluding side cover
2.	Weight			Approx. 155 g { 0.34 lbs.} 
3.	Construction material
a.	Main body		ABS/PC resin
4.	Finish
a.	Main body		i-PRO white

K.	ENVIRONMENTAL
1.	Operating Temperature	-10 °C to +50 °C (14 °F to 122 °F)                                                                                                                                              
2.	Operating Humidity	 10 % ~ 90 % (without condensation)