i-PRO WV-S3532LM FIXED DOME NETWORK CAMERA 
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2004 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd.
B.	Provide Video Surveillance Camera from single source manufacturer

2.2	i-PRO WV-S3532LM COMPACT FIXED DOME NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Fixed Dome Camera shall deliver H.265 stream and H.264 stream. 

2.	The Compact Fixed Dome Camera shall produce a resolution of 1,920 x 1,080 pixels at up to 60 fps with a 16:9 aspect ratio.

3.	The Compact Fixed Dome Camera shall produce a resolution of 2,048 x 1,536 pixels used by super resolution techniques at up to 30 fps with a 4:3 aspect ratio.

4.	The Compact Fixed Dome Camera shall utilize an approximate 1/3 type high sensitivity CMOS image sensor. 

5.	The Compact Fixed Dome Camera shall feature a 144dB wide dynamic range based on Enhanced Compact and Adaptive Black Stretch technology (ABS). 

6.	The Compact Fixed Dome Camera shall produce a color image with a minimum illumination of 0.03 lux and a monochrome image with 0.015 lux at F2.3, shutter speed of 1/30s and AGC11.

7.	The Compact Fixed Dome Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 15m (49feet) irradiation distance.

8.	The Compact Fixed Dome Camera shall equip with M12 connector which can withstand the vehicular vibration and compatible with Railway applications since these cameras comply with ECE-R10.

9.	The Compact Fixed Dome Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and up to three (3) JPEG streams.

10.	The Compact Fixed Dome Camera shall be equipped with intelligent auto mode, the technology for shooting license plate and person’s face more clearly.

11.	The Compact Fixed Dome Camera shall be equipped with GOP control included frame rate control and Smart Facial coding which control an image quality of a stationary area, a moving area and a face, as bitrate reducing technology.

12.	The Compact Fixed Dome Camera shall with corridor mode enables the capture of a more
vertically-oriented area than the normal format would allow.

13.	The Compact Fixed Dome Camera shall produce encrypted stream.

14.	The Compact Fixed Dome Camera shall realize SSL / TLS communication with CA certificate.

15.	The Compact Fixed Dome Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress.

16.	The Compact Fixed Dome Camera shall be rated to IK10 vandal resistance. 

17.	A user shall be able to view video on a PC using a browser.

18.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

19.	The Compact Fixed Dome Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size. 

20.	The Compact Fixed Dome Camera shall offer an optional intelligent VMD (i-VMD) which provides intruder detection, loitering detection, direction detection, scene change detection, object detection and cross line detection.

21.	The Compact Fixed Dome Camera shall have up to 4x digital zoom function. 

22.	The Compact Fixed Dome Camera shall have Fog compensation function.

23.	The Compact Fixed Dome Camera shall have High light compensation (HLC) function.

24.	The Compact Fixed Dome Camera shall have Lens Distortion Compensation to compensate the barrel distortion. 

25.	The Compact Fixed Dome Camera shall provide up to eight (8) areas of electronic privacy masking. 

26.	The Compact Fixed Dome Camera shall offer the prioritized stream control which transmits a video stream to the specified client PC or recorder preferentially. 

27.	The Compact Fixed Dome Camera shall have three (3) alarm sources of  VMD, Panasonic alarm command and  audio detection alarm that activate the processes such as microSDXC/SDHC/SD memory recording, FTP image transfer, E-mail notification, HTTP alarm notification, Indication on browser, and  TCP alarm notification output. 

28.	The Compact Fixed Dome Camera shall have a microSD memory card slot that supports microSD, microSDHC and microSDXC memory card for local storage. 

29.	The Compact Fixed Dome Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/3 type CMOS image sensor
2.	Effective Pixels                  Approx. 2.4 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.03 lux (F2.3, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.0 lux (with IR LED on)
0.015 lux (F2.3, Maximum shutter: Off(1/30s), AGC: 11)

5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		144 dB typ. (Super Dynamic: On)
7.	Built-in IR illumination
a.	Irradiation distance	Approx. 15m (49feet)
C.	Lens
1.	Focal Length		2.8 mm (1/8 inches)
2.	Max. Aperture Ratio	1 : 2.3
3.	Angular Field of View
a.	16:9 aspect ratio	H: 108°,    V: 60°               
b.	 4: 3 aspect ratio	H:   89°,    V: 66°
               4.     Adjusting Angle                 
                                                                Horizontal (PAN) angle : ±45°
Vertical (TILT) angle     : 0 to +90° *
*When viewing images at night using IR LED, set the vertical
(TILT) angle between 0 ° to +75°
Azimuth (YAW) angle   : ±90°.

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio (2 mega pixel mode) (30/60fps)
1,920 x 1,080 / 1,280 x 720 / 640 x 360 / 320 x 180 
b.	4:3 aspect ratio (3 mega pixel mode) (30fps)
2,048 x 1,536* / 1,280 x 960 / 800 x 600 / 640 x 480 / 400 x 300 /
320 x 240
*Used by super resolution techniques
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate, VBR, Frame rate, Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 / 60 fps
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1,024 / 1,536 / 2,048 / 3,072 / 
4,096 / 6,144 / 8,192 / 10,240 / 12,288 / 14,336 / 16,384 / 
20,480 / 24,576 / 30,720 / 40,960 kbps
d.	Image Quality	
i.	Constant bit rate	Motion priority / Normal / Quality priority
ii.	Frame rate            Motion priority / Normal / Quality priority
iii.	Best effort	Motion priority / Normal / Quality priority
iv.	VBR		10 steps
e.	Transmission type	Unicast, Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
H.264                        Off / On(Low) / On(Mid) 
H.265                        Off / On(Low) / On(Mid) / On(Advanced) / On(Frame rate control)  
                        b.   Smart Facial Coding  Off / On(AUTO VIQS) / On(Smart Facial Coding)
*Smart Facial Coding is only available with Stream(1).
E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 /  64 kbps

F.	OPERATION
1.	Super Dynamic		On / Off  
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	On / Off 
4.	Fog compensation	On / Off
                                          (only when Intelligent auto / auto contrast adjust : Off)

5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off   (Only when Super dynamic and Intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Shutter Speed		Max. 1/10000 s to Max. 16/30 s
8.	Day & Night		Off/ On(IR Light Off)/ On(IR Light On)/ Auto1(IR Light Off)/
Auto2(IR Light On)/ Auto3(SCC)
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Privacy Zone		On / Off, Up to 8 zones
12.	Camera Title (OSD)	Up to 20 characters (alphanumeric characters, marks)
13.	Digital Zoom		1x, 2x, 4x
14.	Lens Distortion Compensation	256 steps

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, M12 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, FTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, LLDP, SSL/TLS, SFTP, MQTT
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, FTP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ, LLDP, SSL/TLS, SFTP, MQTT
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

H.	INTERFACE
1.	Microphone input		Built-in microphone
2.	SD memory card slot	1 slot, microSD/SDHC/SDXC

I.	ELECTRICAL
1.	Power Source		PoE (DC48V/80mA, Class 0)
2.	Power Consumption	Approx. 3.8W(PoE)

J.	SAFETY / EMC
1.	Safety			UL (UL60950-1 2Ed), c-UL (CAN/CSA C22. NO.60950-1-07),
CE, IEC60950-1,EN45545-2 compliant, NFPA130, ECE-R118
2.	EMC 			FCC (Part15 Subpart B, ClassA, SDoC), ICES-003 ClassA,
EN55032 ClassB, EN55024, ECE-R10, EN50498, EN50121

K.	MECHANICAL
1.	Dimensions (D x H)	ø109 mm x 53 mm (H) {ø4-9/32 inches x 2-3/32 inches (H)}
2.	Weight			Approx. 410 g (0.91 lbs.)
3.	Construction material
a.	Main body		Aluminum die cast
b.	Dome section	Polycarbonate resin
4.	Finish
a.	Main body		Light gray
b.	Dome section	Clear

.
L.	ENVIRONMENTAL
1.	Vandal Resistance	IEC 62262 IK10
2.	Ingress Resistance	IP66, IEC60529 measuring standard compatible, 
Type 4X (UL50), NEMA 4X compliant
3.	Railway Application	EN50155 : 2017 Class OT2/ST2 (EN 50155 : 2007 Class TX),
 IEC62236-3-2)
4.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F)
5.	Operating Humidity	 10 % ~ 100 % (without condensation)

M.	SOFTWARE OPTIONS
1.	Extension Software for intelligent Video Motion Detection  WV-SAE200